NOTES ON One Per Desk SERVPAK

Opening screen

V5,3 Factory Tutor 1.4

Type HELP

Next Screen

BF BM BR NOBR BS BT CC DC

DF DP DU G GD GO GT HE

LO M MD MM MS OF PF T

T1 TM TR TT VE

BF – Syntax error

BM – Ser

BR – Breakpoints?

NOBR Breakpoints?

BS – Ser

BT – Ser

CC – CMOS Configurator

 1 UK OPD

 2 UK TONTO

 3 Australia

 4 South Africa

 5 New Zealand

 6 /

7 /

DC – Syntax Error

DF – Memory dump?

DP – Confidence Tests

0 – DRAM

1 – SRAM

2 – Monitor

3 – Keyboard

4 – Telephony

5 – Voice Synth

6 – Printer

7 – Microdrives

8 – Auxilary

9 – System Test

X – Return

DU – Syntax Error

GD – No response

GO - No response

GT - Syntax Error

HE – List of Memory address?

LO – OPD locked up

M - Syntax Error

MD – Memory dump at 000000

MM - Syntax Error

MS - Syntax Error

OF – Dump of Memory address R0 to R7?

PF –

 FORMAT = 1515

 CHAR NULL = 0000

 C/R = 0000

 OPTIONS@0281AA

T – Physical Address 00000000

TM - \*TRANSPARENT\* EXIT $01 = CTLA OPD LOCKED UP

TR – Seems same as T

TT - Syntax Error

VE – OPD Locked up