NeXTSTEP Driver Compatibility Guide

TOPIC

This document describes in general terms the types of PC-compatible hardware supported by NeXTSTEP Release 3.3. This document also provides lists of specific drivers available for NeXTSTEP. For more detail on a driver, click on the driver name.

NOTE: Apple Enterprise Software has suspended on-going development of new drivers for the NeXTSTEP and OPENSTEP product lines. Where possible, we will be updating current drivers for minor product revisions. These drivers will be made available in the TIL.

If you have specific requirements for drivers for hardware not currently supported, contact your AES sales representative for a quote for custom development work.

DISCUSSION

OVERVIEW

This guide is divided into six sections:

General System Requirements

Display Options

Networking Options

SCSI Options

Sound Options

System Options

GENERAL SYSTEM REQUIREMENTS

CPU

486, Pentium, or Pentium, Pro based PC compatible computer. NeXTSTEP requires a floating-point coprocessor. Systems using processors without a built-in floating-point coprocessor require an add-on floating-point coprocessor, or upgrade to a 486, Pentium or Pentium Pro with built-in floating-point support.

EXPANSION BUS

ISA, EISA, VL-Bus or PCI expansion bus.

AVAILABLE HARD DISK SPACE

NEXTSTEP supports multiple partitioned hard disks, allowing the user to install and boot several operating systems from the same local hard disk. Larger local disks are recommended for stand-alone systems or for systems with a local non-NEXTSTEP partition.

User Environment:120 MB partition minimum, 200 MB recommended for stand-alone systems.

User + Developer: Environments: 330 MB partition minimum, 400 MB recommended.

RAM REQUIREMENTS

RAM requirements vary depending upon your selection of graphics adapter and imaging model.

32-bit color: 24 MB RAM Minimum, 32 MB RAM Recommended

16-bit color: 16 MB RAM Minimum, 24 MB RAM Recommended

8-bit color/grayscale: 12 MB RAM Minimum, 16 MB RAM Recommended

2-bit grayscale: 8 MB RAM Minimum, 12 MB RAM Recommended

GRAPHICS ADAPTERS

See the "Display Options" section in this guide for details on graphics support.

DISK INTERFACES

IDE and several SCSI hard disk interfaces are supported.

POINTING DEVICES

Microsoft(tm) and Logitech(tm) compatible PS/2(tm) and serial mice. Logitech bus mouse.

PRINTERS

Any PostScript printer connected via a serial port, parallel port or network including the NeXT Color Printer (connected via a SCSI port). Apple Computer recommends color PostScript printers with PostScript Level II for proper color support.

NETWORKING

Several Ethernet and Token Ring networking adapters are supported. A networking adapter is optional.

SOUND

NEXTSTEP can support certain PC sound cards for both playback and recording. A sound card is optional.

DISPLAY OPTIONS

_ATI_
- ATI Graphics Ultra Pro (EISA, ATI 68875 RAMDAC)
- ATI Graphics Ultra Pro (EISA, TI 34075 RAMDAC)
- ATI Graphics Ultra Pro (VL-Bus, ATI 68875 RAMDAC)
- Intel GX/Pro (Custom LB, onboard ATI, TI 34075 RAMDAC)
- Data General Dasher DE2 (Custom LB, TI 34075 RAMDAC)
- AST Premmia 4D (Custom LB, onboard ATI, BT 481 RAMDAC)
- Gateway V Series (VL-Bus, ATI 68875 RAMDAC)

_ATI Mach32_
- ATI Graphics Ultra Pro - EISA (with 2MB VRAM)
- ATI Graphics Ultra Pro - PCI (with 2MB VRAM)
- ATI Graphics Ultra Pro - VL-Bus (with 2MB VRAM)
- ATI Graphics Ultra Pro XLR - VL-Bus (with 2MB DRAM) - not tested, but should work
- ATI Graphics Ultra Pro XLR - PCI (with 2MB DRAM) - not tested, but should work
- Intel GX/Pro (Custom LocalBus, onboard ATI, TI 34075 RAMDAC)
- Data General Dasher DE2 (Custom LocalBus, TI 34075 RAMDAC)
- AST Premmia 4D (Custom LocalBus, onboard ATI, BT 481 RAMDAC)
- Gateway V Series (VESA LocalBus, ATI 68875 RAMDAC)

_ATI Mach64_
- ATI Graphics Ultra Pro Turbo (PCI, with 2MB VRAM)
- ATI Graphics Ultra Pro Turbo (PCI, with 2MB DRAM)
- ATI Graphics Ultra Pro Turbo (PCI, with 4MB VRAM)
- ATI Graphics Ultra Pro Turbo (PCI, with 4MB DRAM)
- ATI Graphics Ultra Pro Turbo (VL-Bus, with 4MB VRAM)
- ATI Graphics Ultra Pro Turbo (VL-Bus, with 4MB DRAM)
- AT&T Globalyst 600

_ATI Rage_
- ATI All-In-Wonder
- ATI 3D Pro Turbo
- ATI 3D Pro Turbo PC2TV
- ATI 3D Xpression+
- ATI 3D Xpression+ PC2TV
- ATI XPERT @ Work
- ATI XPERT @ Play

_Canon object.station41 Display_
- Canon object.station 41

_Chips & Technologies Wingine_
- Epson Wingine
- LGI Wingine

_Chips & Technologies Wingine 64300_
- NEC Powermate 466D

_Cirrus Logic GD542X Family_

_Cirrus Logic GD5434_
- Diamond SpeedStar 64 (PCI)
- Orchid Kelvin 64 (with GD5434)
- Elonex WS4100
- Intel Premier (with integrated GD5434)
- HP Vectra XM Series3 (not tested but reported to work)

_Compaq QVision_
- QVision 1024/E EISA (QV30E, QV32E)
- QVision 1280/E EISA (QV32E)
- QVision 1280/P PCI (QV35P, QV64P)
- Compaq Deskpro XE560
- Compaq Deskpro XE466
- Compaq Deskpro 5100

_Dell DGX (JAWS)_
- Dell 450DE/2 DGX

_Diamond Stealth_
- Diamond Stealth 64 DRAM PCI-Bus Display Adapter
- Diamond Stealth 64 DRAM VL-Bus Display Adapter
- Diamond Stealth 64 Video PCI-Bus Display Adapter
- Diamond Stealth 64 Video VL-Bus Display Adapter
- Diamond Stealth 64 VRAM PCI-Bus Display Adapter
- Diamond Stealth SE PCI-Bus Display Adapter
- Diamond Stealth SE VL-Bus Display Adapter
- Diamond Stealth 64 DRAM T PCI-Bus Display Adapter
- Diamond Stealth 64 DRAM T VL-Bus Display Adapter
- Diamond Stealth 64 Video VRAM VL-Bus Display Adapter
- Diamond Stealth 64 Video 3200 VL-Bus Display Adapter
- Diamond Stealth 64 Video 2121XL DRAM PCI-Bus Display Adapter
- Diamond Stealth 64 Video 3000 VRAM PCI-Bus Display Adapter
- Diamond Stealth 3D 2000 PCI-Bus Display Adapter
- Diamond Stealth 3D 3000 PCI-Bus Display Adapter

_Diamond Stealth64_
- Diamond Stealth 64 (PCI, 4MB VRAM)
- Diamond Stealth 64 (PCI, 2MB VRAM)
- Diamond Stealth 64 (VL-Bus, 4MB VRAM)
- Diamond Stealth 64 (VL-Bus, 2MB VRAM)

_HP Vectra XP_
- HP Vectra XP (4MB VRAM)
- HP Vectra XP (2MB VRAM)

_HP Vectra XU Display_
- HP Vectra/XU S3/864 on-board video

_IBM ThinkPad 755CX Display_
- IBM ThinkPad 755CX

_IBM ThinkPad 760CD Display_
- IBM ThinkPad 760CD

_IBM ThinkPad 760ED Display_
- IBM ThinkPad 760E
- IBM ThinkPad 760ED
- IBM ThinkPad 560

_Matrox MGA Millennium_
- Matrox MGA Millennium
- Matrox MGA Millennium II
- Matrox MGA Millennium II AGP
- Matrox Mystique
- Matrox Mystique 220
- Matrox Mystique 220 AGP

_Number Nine GXE Family_
- #9GXE-VL Level 10 (VL-Bus, 1MB VRAM) - not tested, but should work
- #9GXE-VL Level 11 (VL-Bus, 2MB VRAM)
- #9GXE-VL Level 12 (VL-Bus, 2MB VRAM) - not tested, but should work
- #9GXE-VL Level 14 (VL-Bus, 4MB VRAM) - not tested, but should work
- #9GXE-VL Level 16 (VL-Bus, 4MB VRAM) - not tested, but should work
- #9GXE-PCI Level 10 (PCI, 1MB VRAM) - not tested, but should work
- #9GXE-PCI Level 12 (PCI, 2MB VRAM)

_Number Nine GXE64 Pro_
- Number 9 GXE 64 Pro (PCI, 4MB VRAM)
- Number 9 GXE 64 Pro (PCI, 2MB VRAM)
- Number 9 GXE 64 Pro-1600 (PCI, 4MB VRAM, 200Mhz RAMDAC) - not tested, but should work
- Number 9 GXE 64 Pro (VL-Bus, 4MB VRAM)
- Number 9 GXE 64 Pro (VL-Bus, 2MB VRAM)
- Number 9 GXE 64 Pro-1600 (VL-Bus, 4MB VRAM, 200Mhz RAMDAC) - not tested, but should work

_Number Nine Imagine128_
- Number9 Imagine 128 (PCI) (NB128-V2-P)

_Number Nine Imagine128 Series 2_
- Number9 Imagine 128 Series 2 (4MB) (90-228120-000)
- Number9 Imagine 128 Series 2 (8MB) (90-228130)
- Number9 Revolution 3D (4MB)
- Number9 Revolution 3D (8MB)

_Number Nine Motion331_
- Number Nine 9FX Motion 331 1MB PCI (NB9-FX1-331-1P)
- Number Nine 9FX Motion 331 2MB PCI (NB9-FX1-331-2P)

_Number Nine Motion771_
- Number Nine 9FX Motion 771 2MB PCI (NB9FX2-771-2P)
- Number Nine 9FX Motion 771 4MB PCI (NB9FX2-771-4P)
- Number Nine 9FX Motion 771 2MB VL-Bus (NB9FX2-771-2VL)
- Number Nine 9FX Motion 771 4MB VL-Bus (NB9FX2-771-4VL)

_S3 805 / 928_
- IBM PS/ValuePoint
- Hewlett-Packard Vectra XM
- DECpc 466d2 MTE

_S3 Generic_

_S3 ViRGE Display Driver_
- Number Nine 9FX Reality 332 PCI Display Adapter (90-332010-000, 91-332010-000, 91-332013-000)
- Diamond Stealth 3D 2000 PCI Display Adapter

_STB Pegasus_
- STB Pegasus (VL-Bus, 4MB VRAM)
- STB Pegasus (VL-Bus, 2MB VRAM)

_Trident Generic_
- This driver will not support the built-in display on IBM Thinkpad 760CD.

_Tseng Labs ET4000_

_Tseng Labs ET4000W32_

_VGA_

_Weitek Power 9000_
- Diamond Viper (PCI)
- Diamond Viper (VL-Bus)
- Genoa VideoBlitz 9200-VL (VL-Bus) - not tested, but should work

_Weitek Power 9100_
- Diamond Viper Pro (PCI, 2MB VRAM)
- Diamond Viper Pro (PCI, 4MB VRAM)

_Western Digital WD90C24_
- NEC Versa E Series
- NEC Versa V Series
- Compaq LTE Elite

NETWORKING OPTIONS

_3COM EtherLink III_
- 3Com EtherLink III 3C509 ISA (BNC, AUI)
- 3Com EtherLink III 3C509B ISA (BNC, AUI)
- 3Com EtherLink III 3C509-TP ISA (RJ-45, AUI)
- 3Com EtherLink III 3C509B-TP ISA (RJ-45, AUI)
- 3Com EtherLink III 3C509-COMBO ISA (BNC, AUI, RJ-45)
- 3Com EtherLink III 3C509B-COMBO ISA (BNC, AUI, RJ-45)
- 3Com EtherLink III 3C509-TPO ISA (RJ-45)
- 3Com EtherLink III 3C509B-TPO ISA (RJ-45)
- 3Com EtherLink III 3C579 EISA (BNC, AUI)
- 3Com EtherLink III 3C579-TP EISA (AUI, RJ-45)
- 3Com EtherLink III 3C589C-COMBO (BNC, RJ-45)
- 3Com EtherLink III 3C589C-TP (RJ-45)

_3COM EtherLink XL_
- 3Com EtherLink XL 3C900-TPO PCI (RJ-45)
- 3Com EtherLink XL 3C900-Combo PCI (BNC, AUI, RJ-45)
- 3Com EtherLink XL 3C905-TX PCI (10Base-T, 100Base-TX)
- 3Com EtherLink XL 3C905B-TX PCI (10Base-T, 100Base-TX)

_AMD PCnet32_
- X/Lan Add-On Adapter (based on Am79C970).
- Canon object.station 41
- Compaq Deskpro XL (On-board)
- HP Vectra XU (On-Board)

_Cogent EM960 PCI_
- Cogent EM960C (PCI, Combo)
- Cogent EM960TP (PCI, TP Only)
- Cogent EM964TP (PCI, TP Only, 4 ports - 1st port only supported)

_Cogent EMaster EISA_
- EM932 (EISA, BNC/AUI)
- EM932TP (EISA, UTP/AUI)
- EM935XL (EISA, BNC/UTP/AUI)

_DEC21142Network_
- DEC Celebris 61xx On-Board LAN Adapter

_DEC21X4XNetwork_
- Adaptec-Cogent ANA-6911A/TX
- Cogent EM110-TX Fast Ethernet 10/100 Adapter
- Cogent EM960 PCI
- DEC DE500 (21143 based) PCI 10/100
- DEC DE500 Fast EtherWORKS PCI 10/100
- DANPEX PCI Ethernet (EN-9400P3)
- SMC 9332 Fast Ethernet 10/100 Adapter
- SMC PCI EtherPower (SMC 8432)
- DEC Celebris GL On-Board LAN Adapter (21142/21143, 10 Mb/s module)
- DEC Celebris GL On-Board LAN Adapter (21142/21143, 10/100 Mb/s module)

_DECchip21040 Network_
- Cogent EM960 PCI
- SMC PCI EtherPower (SMC 8432)
- Digital EtherWORKS Turbo PCI (DE435)
- Linksys EtherPCI LAN Card
- DANPEX PCI Ethernet (EN-9400P3)
- JCIS Condor (JC1260)
- Kingston EtheRx PCI Ethernet (KNE40T & KNE40BT)
- DEC Celebris GL & GLST

_DECchip21140 Network_
- Cogent EM100 Fast Ethernet Adapter
- Cogent EM110 Fast Ethernet 10/100 Adapter
- Cogent EM110-T4 Fast Ethernet 10/100/BNC Adapter
- DEC DE500 Fast EtherWORKS PCI 10/100
- SMC 9332 Fast Ethernet 10/100 Adapter
- SMC EtherPower 10/100 B Fast Ethernet Network Adapter (9332BDT)

_HP Vectra XM, XP Integrated_
- HP Vectra XM
- HP Vectra XP
- Elonex WS4100 - Not tested, should work

_IBM Token Ring_
- IBM 25F7367 (ISA, 16/4 Mbps, 8-bit, 64K)
- IBM 25F9858 (ISA, 4Mbps, 8-bit, 16K)
- IBM 67X0438 (ISA, 4Mbps, 8-bit, 16K)
- IBM 60G3994A? (ISA, 16/4 Mbps, 16-bit, 64K)
- IBM 92G7668 (Auto, ISA, 16/4 Mbps, 16-bit, 64K)
- IBM 41H8450 (Auto, ISA, 16/4 Mbps, 16-bit, 64K)
- Token Ring option for Compaq DeskPro and Prolinea series

_Intel 82556 Network_
- Intel EtherExpress PRO/100 EISA LAN Adapter (EILA8265)
- Intel EtherExpress PRO/100 PCI LAN Adapter (PILA8465)

_Intel 82557 Network_
- Intel EtherExpress PRO/100+ PCI LAN Adapter (10Base-T, 100Base-TX)
- Intel EtherExpress PRO/100 PCI LAN Adapter (PILA8465B) (10Base-T, 100Base-TX)
- Intel EtherExpress PRO/100 PCI LAN Adapter (PILA8475B) (10Base-T, 100Base-T4)
- Intel EtherExpress PRO/10+ PCI LAN Adapter (PILA8500) (BNC, AUI, RJ-45)
- Intel EtherExpress PRO/10+ PCI LAN Adapter (PILA8520) (RJ-45)

_Intel 82595 Chipset_
- Cogent EM595 TP PCMCIA (RJ-45)
- Cogent EM595 C PCMCIA (RJ-45/BNC)
- Intel EtherExpress PRO/10 ISA LAN Adapter (BNC/RJ-45/AUI)
- Intel EtherExpress PRO/10+ ISA LAN Adapter (BNC/RJ-45/AUI) (PCLA8200B)
- Intel EtherExpress PRO/10+ ISA LAN Adapter (BNC/RJ-45) (PCLA8210B)
- Intel EtherExpress PRO/10+ ISA LAN Adapter (RJ-45) (PCLA8220B)
- Intel EtherExpress PRO/10+ ISA LAN Adapter (BNC/RJ-45/AUI) (PCLA8205B)
- Intel EtherExpress PRO/10+ ISA LAN Adapter (BNC/RJ-45) (PCLA8215B)
- Intel EtherExpress PRO/10+ ISA LAN Adapter (RJ-45) (PCLA8225B)

_Intel 82596 Network_
- Intel EtherExpress PRO/10 PCI (PILA8400) (BNC, UTP, AUI)
- Intel EtherExpress PRO/10 PCI (PILA8420) (UTP)
- Intel EtherExpress Flash32 EISA (EILA8225) (BNC, UTP, AUI)
- Cogent eMaster EM935 EISA XL (BNC, UTP, AUI)
- Cogent eMaster EM932 EISA (UTP, AUI)
- Cogent eMaster EM932 EISA (BNC, UTP, AUI)
- Cogent eMaster EM945 EISA FDE (BNC, UTP, AUI)

_Intel EtherExpress16_
- EtherExpress16 (ISA, BNC/AUI)
- EtherExpress16TP (ISA, UTP/AUI)
- EtherExpress16C (ISA, BNC/UTP/AUI)

_Intel TokenExpress_
- STP (ISA)

_SMC EtherEZ/Elite16 Ultra_
- SMC EtherCard Elilte Ultra16 (ISA)
- SMC EtherCard Elilte Ultra16T (ISA)
- SMC EtherCard Elilte Ultra16C (ISA)
- SMC EtherEZ (8416BTA)
- SMC EtherEZ (8416B)
- SMC EtherEZ (8416T)
- SMC EtherEZ (8416BT)
- SMC EtherEZ (8416BA)
- SMC EtherEZ (8416TA)

_SMC EtherElite 16_
- SMC EtherCard Plus Elite16 Ethernet Adapter

_Xircom Netwave_
- Xircom CreditCard Netwave Adapter (CNW(AM))

_Xircom Performance Series_
- Xircom PS-CE2-10BT (PCMCIA, UTP)
- Xircom PS-CE2-10BC (PCMCIA, UTP/BNC)

SCSI OPTIONS

_AMD PC SCSI_
- Toshiba CD-ROM XM-3401T
- Peripheral Solutions 8mm Exabyte DAT Drive -- 8500
- Syquest 88MB SQ5110 D3G 810
- IOMEGA Bernoulli 230 BETA230 1.1408/2
- Pinnacle Micro Tahoe 230MB MO J6CTahoe-130A
- Quantum 504MB LPS5255S 311012 Hard Drive
- Quantum LPS540S 590H01 Hard Drive
- Next SCSI Color Printer
- HSD Scan-X Color Scanner (UMAX engine)
- COMPAQPC DPES-31080
- Compaq Deskpro XL
- HP Vectra XU

_Adaptec 154x family and compatible_
- Adaptec 154xB (ISA)
- Adaptec 154xC (ISA)
- Adaptec 154xCF (ISA)
- Adaptec 174x (EISA) in standard 154x mode only

_Adaptec 274x and 284x family_
- Adaptec 2740 (EISA) - not tested but should work
- Adaptec 2740T (EISA)
- Adaptec 2840 (VLB)

_Adaptec 2940 family & 7870 integrated_
- Adaptec AHA-2930B (PCI)
- Adaptec AHA-2940 (PCI)
- Adaptec AHA-2940W (PCI, Wide SCSI)
- Adaptec AHA-2940U (PCI, Ultra SCSI)
- Adaptec AHA-2940UW (PCI, Ultra/Wide SCSI)
- Adaptec AHA-2910B (PCI) - Not tested but should work.
- DEC EISA/PCI Server system w/ 7870 on motherboard
- DEC Celebris GLST w/ 7850 on riserboard
- HP Kayak on-board 7860 & 7880 based SCSI adapters.

_Adaptec 6x60 chipset (add-on & integrated)_
- Adaptec AVA-1505A (ISA)
- Adaptec AVA-1515A (ISA)
- Adaptec AHA-1520A (ISA)
- Adaptec AHA-1530P (ISA) - Not tested but might work.
- Adaptec Slim SCSI (PC/MCIA)
- Intel GX/Pro

_Bus Logic FlashPoint_
- BusLogic KT-930 PCI SCSI Host Adapter
- BusLogic KT-932 PCI Dual Chanel SCSI Host Adapter
- BusLogic BT-950 PCI Wide SCSI Host Adapter

_BusLogic family_
- BusLogic 546C ISA SCSI Host Adapter
- BusLogic 747C EISA SCSI Host Adapter
- BusLogic 445C VL-Bus SCSI Host Adapter
- BusLogic 946C PCI SCSI Host Adapter (rev C and D only)
- BusLogic 948 PCI SCSI Host Adapter (not tested, reported to work)
- BusLogic 958 PCI Wide SCSI Host Adapter (not tested, reported to work)
- Canon object.station 41

_DPT 2000 family_
- DPT 2021/9x SmartCache III (ISA) - not tested, but should work
- DPT 2022/9x SmartCache III (EISA)
- DPT 2122/9x SmartCache III (EISA)
- DPT 2122/9xW SmartCache III (EISA, Wide) - not tested, but should work
- DPT 2122/9xDW SmartCache III (EISA, Differential, Wide) - not tested, but should work
- DPT 2024 SmartCache III (PCI) - In future update
- DPT 2124 SmartCache III (PCI) - In future update
- NEC Express II P60 (On-Board)

_DPT SCSI family_
- PM2021/90 ISA SCSI adapter
- PM2021/95 ISA SCSI adapter
- PM2022/90 EISA SCSI adapter
- PM2022/95 EISA SCSI adapter
- PM2024 PCI SCSI adapter
- PM2041W ISA Wide SCSI adapter (not tested)
- PM2042W EISA Wide SCSI adapter (not tested)
- PM2044W PCI Wide SCSI adapter (not tested)
- PM2122/90 EISA SCSI adapter
- PM2122/95 EISA SCSI adapter
- PM2124 PCI SCSI adapter
- PM2124W PCI WIDE SCSI adapter
- PM2142W EISA Wide SCSI adapter (not tested)
- PM3021 ISA SCSI RAID controller (Not tested, should work)
- PM3222 EISA SCSI RAID controller
- PM3224 PCI SCSI RAID controller
- DPT-TWR n/a 6-bay SCSI Tower
- DPT-TWR/W n/a 6-bay WIDE SCSI Tower (Not tested, should work)
- NEC Express II P60 (On-Board)

_SymbiosLogic53C8xxSCSIDriver_
- DEC Celebris XL/590

SOUND OPTIONS

_Beep_

_Canon object.station41 Sound_
- Canon object.station 41

_Compaq Business Audio_
- Compaq Deskpro / M
- Compaq Deskpro / I

_ESS 1x88 Audio Driver_
- NewCom High Fidelity 16i E5X1853
- Compaq Prolinea
- NEC Versa 4000
- DEC Celebris GL & GL/ST

_IntelGXProAudio_
- Intel GX/Professional

_Media Vision Jazz 16_
- Media Vision Deluxe Sound Card
- Media Vision Pro Sonic Sound Card

_Microsoft Sound System_
- Microsoft Sound System (ISA)

_Pro Audio Spectrum 16_

_Sound Blaster 16_
- Sound Blaster 16 Basic (ISA)
- Sound Blaster 16 Value (ISA)
- Sound Blaster 16 AWE (ISA)
- Sound Blaster 16 SCSI-II (ISA)
- Sound Blaster 16 Value PnP (ISA)
- Sound Blaster AWE 64 Value (ISA)
- Sound Blaster AWE 64 Gold (ISA)

_Sound Blaster 8_
- Sound Blaster Basic ISA)
- Sound Blaster Pro (ISA)
- Sound Blaster Delux (ISA)
- Sound Blaster Value (ISA)

_Yamaha OPL Audio_
- Yamaha OPL3-SA3 (YMF715) based PNP audio adapters
- Yamaha OPL3-SA (YMF701B) based on-board audio adapters

SYSTEM OPTIONS

_BusMouse_
- Logitech MouseMan Bus
- Logitech MouseMan Cordless

_EIDE_

The following ATAPI CD-ROM drives are supported:
- Chinon CD-ROM CDS-525 (2X), firmware rev. W09
- Matsushita CD-ROM CR-571 (2X), firmware rev. 1.0e -- Panasonic
- Mitsumi CD-ROM 1B (4X), firmware rev. B02 -- model FX400
- Sony CD-ROM CDU55E (2X), firmware rev. 1.0u
- Sony CD-ROM CDU76E-S (4X), firmware rev. 1.0c
- Toshiba CD-ROM XM-5302TA (4X), firmware rev. 0305
- Philips CM207, firmware rev 1.10 (??) -- reported to work
- SONY CD-ROM CDU76E-Q, firmware rev 1.0c (4X)
- SONY CD-ROM CDU55D, firmware rev 1.0v (2X)
- SONY CD-ROM CDU77E, firmware rev 1.0e (4X)
- TORiSAN CD-ROM CDR-S1, firmware rev 1.70 (4X) -- SANYO
- Chinon CD-ROM CDS-545, firmware rev ERc A1.0 (4X)
- GoldStar CD-ROM GCD-R540, firmware rev 1.17 (4X)
- GoldStar CD-ROM GCD-540C, firmware rev 1.01 (4X)
- SANYO CRD-254P, firmware rev 1.02 (4X)
- MATSHITA CD-ROM CR-574, firmware rev 1.06 (4X) -- Panasonic
- Pioneer CD-ROM DR-UA124X, firmware rev 1.02 (4X) -- force detection
- MITSUMI CD-ROM !B, firmware rev K02 (4X) -- DRM FX400B
- TEAC CD-55E, firmware rev ?? (4X) -- Thinkpad 760CD
- ATAPI CD-ROM SPEED-6X, firmware rev 6.2D (6X) -- ACER 665A
- VERTOS 600ESD CD-ROM X6-IDE, firmware rev 1.20 (6X)
- TEAC CD-56E, firmware rev 1.0D (6X)
- MATSHITA UJDCD4700, firmware rev 1.11 (??)
- TEAC CD-58E, firmware rev 1.1B (8X)
- Toshiba CD-ROM XM-5602B, firmware rev 1426 (8X)
- Sony CD-ROM CDU311, firmware rev 3.0i (8X)
- EPSON CMD-2240 SPEED-6X, firmware rev R100 -- reported to work
- Hitachi CDR-7730, firmware 1.1a (4X)
- TEAC CD-524E, firmware 4.0D (24X)

_EISABus_

_Floppy_

_IDE_

_ISA Serial Port_

_Intel 82365 and compatible PCMCIA chipset_
- SwapBox Classic MMCD-D - Not tested, might work.
- NEC Versa E Series
- NEC Versa V Series
- NEC Versa 4000
- Compaq LTE Elite
- IBM Thinkpad 755CX
- Adaptec CardPark

_Intel 824X0 PCI Chipset_

_PCI Bus_

_PCMCIABus_

_PS/2-Style Mouse_
- Rose Electronics ServeView Keyboard/Mouse/Display multiplexer

_PS2Keyboard_

_ParallelPort_

_Port Server_

_SCSITape_

_Serial Pointing Device_
- Alps Glidepoint
- LogiTech FirstMouse
- LogiTech MouseMan
- LogiTech MouseMan Cordless
- LogiTech TrackMan
- Kensington Expert Mouse v2.0
- Kensington Expert Mouse v4.0
- Microsoft Serial Mouse
- Mouse Systems PC Mouse III

_SerialMouse_

_SerialPorts_

OTHER OPTIONS

_FTG ISA Light Pen_
- PXL-395 Light Pen Interface (ISA)
- FT-356 1-Button Light Pen
- FT-357 2-Button Light Pen

_FTG Light Pen_
- PXL-780 Light Pen Interface (Serial)
- FT-356 1-Button Light Pen
- FT-357 2-Button Light Pen